**Microprocessor Systems Design**

**EEE 42101**

**Experiment 2: Timers and Interrupts.**

# Objectives:

* Study Timers and their interrupts.

## Tools:

1. PC
2. Arduino Nano board
3. Testing board
4. MiniB-USB cable

Note: all material and sources of this course will be available on:

<https://github.com/ashrafmalraheem/Mircoprocessor_Course>

Feel free to download, study and modify for your own projects.

# Part 1: Set Timer

Timer is a counter with 8, 16- or 32-bit register it depends on the architecture of the microcontroller unit. It increments its value by one every one clock cycle. The clock of the timer need not to be the same of the core clock. It can be its clock or its clock divided by a certain value. It also can have external clock source. All of this is set by bits on its control registers. You can get and set the value of the timer by accessing its data register. You can also generate interrupt if an overflow occurred. Then you can define an interrupt service routine to perform certain function.

The advantage of using timers is that they are separate device run without the microcontroller core intervention. It can generate interrupts when it has an overflow. Therefore, they can be used as a delay without wasting any of the processor resources(time) Instead of delay function.

To set a timer to Blink LED every **1/2 seconds.** you should firstly decide which timer you should use: 8-bit or 16-bit timers?

**Q: What is the selected value of prescaler? Solve the above equation using 16-bit timer**




Figure Clock Select Bit description

From the prescaler value you obtained above, now you should what bits to set in the timer control register **TCCR1B**.

You can use bit manipulation using bit shift operators with bit mask like this:

TCCR1B |= 1<<CS10; // this will set the CS10 bit to 1

TCCR1B |= 1<<CS11; // this will set the CS11 bit to 1

TCCR1B |= 1<<CS11; // this will set the CS12 bit to 1

**Or:**

TCCR1B |= BIT0; // set bit 0




Figure Timer1 B Control Register

You should enable the overflow interrupt in the timer interrupt mask register **TIMSK1**.




Figure Timer1 Overflow interrupt

Code:

TIMSK1 |= 1<<TOIE1; // enable overflow interrupt

Now you should define what is in your interrupt service routine. What the interrupt should do after it occur. You can either set the LED on or off inside this routine. Or you can set a flag to 1 or 0 and then use this flag to turn the LED.

ISR(TIMER1\_OVF\_vect){ // interrupt service routine for timer1 overflow

/\* Replace with your interrupt service routine \*/

}